EASE - Energy-saving-Automated Sauna Experience

Group members

Joonas Salminen

Toni Martikainen

Jayden

Edson

Idea and motivation

Some background:

Social and Economic problem:

Many people die in Sauna (Over staying, Hyperthermia, drunk and being unconsciousness, etc) - 30-40 deaths in Finland 1)http://www.stat.fi/til/ksyyt/2013/ksyyt_2013_2014-12-30_kat_005_en.html

Electric prices going up every year

Global economy in poor condition

Evolution of EU-28 and EA electricity prices for household consumers 2)http://ec.europa.eu/eurostat/statistics-explained/index.php/Electricity_price_statistics

Our scenario is a person trying to save energy/money when using the sauna in a single-person apartment. Our motivation for this comes from the fact that electric sauna stove is one of the biggest electricity consumers at home, about 6-10 kWh/session, with over half of the stove's energy consumption coming from pre-heating and the rest from keeping the warm up during the sauna session. Energy companies usually give some general instructions that you can follow to make the use of sauna more energy-efficient:

Go to sauna immediately when it's ready

Energy-efficient temperature for sauna is 70-80 °C

Avoid breaks between people going to sauna

Avoid keeping the sauna door open

Keep the stove on only during the sauna session

Our idea is to automate some of these to make the person's life easier when trying to save some energy/money. In this case we're going to address points 1 and 2. We're also going to see the how much energy/money a person can save by using motion detection based lights in his sauna.

Features

Basically there are 3 parts in our system:

Alarm system to inform the user when the sauna is ready (due to circumstances the alarm is a switch light turning on when sauna is warm which can then be turned off manually).

Stove heating control which turns the heating on/off as needed to keep the temperature at certain level.

Motion detection based lighting so that lights go on when there is movement and off if there is no movement for certain amount of time.

Scenario 1: Switch on the Sauna and notify the person

Given Switch on the Sauna automatically
When every Tuesday between 19-20.30
Then notifies the person via alarm when temperature in sauna room reaches 70c
And disable alarm automatically

Scenario 2: Turn on the Sauna Lights

Given Sauna is Switched on
When Someone enters the Sauna room
Then turn on the lights

Technology

Automation server: FHEM

Server platform: TuxRadio (Debian/Linux, embedded)

Device protocol: HomeMatic

Used devices:

Temperature sensor

Light bulb

Motion detector

Switches

Energy and cost savings

Calculations are based on the scenario where person uses the sauna 7 times a week for 1.5 h (1 h for warming the sauna to 80 °C and 0.5 h for the sauna session itself) every week during the year.
We assume that the energy costs 0.12 €/kWh which is the average price of household electricity in Finland 3)http://www.vattenfall.fi/fi/keskimaarainen-kulutus.htm. We also assume that the power of the stove is 6 kW and we know that the lamp's power is 0.053 kW.

Stove

Normal situation: Let's assume that without alarm the person would go to sauna 10 minutes later than with alarm and thus waste energy.

6 kW * (1.5 h + 10/60 h waiting time) * 0.12 €/kWh * 52 weeks * 7 = 436.8 € in a year

Our situation:

6 kW * 1.5 h * 0.12 €/kWh * 52 weeks * 7 = 393.12 € in a year

So the saving is about 44 €/year.

Lighting

Normal situation: We assume that the light is on during the heating phase and sauna session itself.

0.053 kW * (1.5 h + 10/60 h waiting time) * 0.12 €/kWh * 52 weeks * 7 = 3.86 € in a year

Our situation: We assume that the motion detecting light is on for 22 minutes (two 4 minute cooldown breaks) during the whole session

0.053 kW * 22/60 h * 0.12 €/kWh * 52 weeks * 7 = 0.84 € in a year

So the saving is about 3 €/year with one lamp.

Total

Thus with our system the total savings are about 47 € (~392 kWh) in a year.

Cost for the equipment:
HomeMatic 131776 Wireless motion detector Indoors: 65 €
HomeMatic 130248 Wireless switch 1-channel Adapter 3680 W: 3 x 54 €
HomeMatic 132095 Wireless temperature and humidity sensor HM-WDS40-TH-I-2 Indoors: 54 €
TUXRADIO : 40 €
Total: 321 €

One time investment. Return of Investment (ROI) : 321/47= 7 years.

Documentation

Project presentation: group2_project_ease.pdf

Protocol presentation: group2_p_enocean.pdf

Project report: This wiki-page

Special challenge report: group2_specialchallengereport.pdf

Project poster: group2_poster.pdf

Sources

scripts.zip

Experiences

Teamwork- awesome

Learned a whole heck of about home automation

Heck of fun to use projector as Sauna

Motivated to install fhem server and install homeMatic devices to control devices and SAVE energy

Learned how to edit front end of fhem server.

Thank you Prof. Dr. Jari Porras and Prof. Dr. Olaf Drögehorn

Overall it was GREAT!!